1.PERFORM SELF-DIAGNOSIS OF ABS ACTUATOR AND ELECTRIC UNIT (CONTROL UNIT) With CONSULT-III Perform“ABS” self-diagnosis. Is DTC detected? YES>>Check the detected DTC items. Refer to DTC No. Index.
NO >>GO TO 2.
2.PERFORM SELF-DIAGNOSIS
With CONSULT-III
Perform “E-SUS” self-diagnosis.
Is another DTC detected?
YES>>Check the detected DTC items. Refer to DTC Index.
NO>>GO TO 3.
3.CHECK INFORMATION
With CONSULT-III
Check ”BRK FLD PRESS” of “DATA MONITOR” for “E-SUS”. Refer to Reference Value (GT-R certified NISSAN dealer).
Is each data within standard values?
YES>>Check pin terminal and connection of each harness connector for damage or loose connection. Repair or replace error-detected parts.
NO >>Replace E-SUS control unit. Refer to Exploded View (GT-R certified NISSAN dealer).