DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
C1105 | RR RH SENSOR-2 | When the distance between the rear RH wheel sensor and sensor rotor is too large and the sensor pulse cannot be recognized by the control unit. |

- Harness or connector
- Wheel sensor
- ABS actuator and electric unit (control unit)

C1106 | RR LH SENSOR-2 | When the distance between the rear LH wheel sensor and sensor rotor is too large and the sensor pulse cannot be recognized by the control unit.
C1107 | FR RH SENSOR-2 | When the distance between the front RH wheel sensor and sensor rotor is too large and the sensor pulse cannot be recognized by the control unit.
C1108 | FR LH SENSOR-2 | When the distance between the front LH wheel sensor and sensor rotor is too large and the sensor pulse cannot be recognized by the control unit.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE

1. Start the engine and drive the vehicle at 30 km/h (19 MPH) or more for approximately 1 minute.
2. Perform self-diagnosis for “ABS” with CONSULT-III.

Is DTC “C1105”, “C1106”, “C1107” or “C1108” detected?
YES>>Proceed to diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END