DTC DETECTION LOGIC

DTC | CONSULT-III display description | DTC detecting condition | Possible cause
B2622 | INSIDE ANTENNA | An excessive high or low voltage from inside antenna is sent to BCM. |

- Inside key antenna (console)
- Between BCM〜Inside key antenna (console)

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Perform inside key antenna (“INSIDE ANT DIAGNOSIS”) on “Work Support” of “INTELLIGENT KEY”.
2. Perform “INTELLIGENT KEY” Self Diagnostic Result.

Is inside key antenna DTC detected?
YES>>Refer to Diagnosis Procedure.
NO>>Inside key antenna (console) is OK.