1.PERFORM INITIALIZATION

1. Perform initialization with CONSULT-III. Reregister all Intelligent Keys.For initialization and registration of Intelligent Key. Refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>GO TO 2.
NO>>INSPECTION END
2.REPLACE INTELLIGENT KEY

1. Replace Intelligent Key. Reregister all Intelligent Keys
2. Perform initialization with CONSULT-III. For initialization, refer to “CONSULT-III Operation Manual NATS-IVIS/NVIS”.
3. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Replace BCM. Refer to Removal and Installation.
NO>>INSPECTION END