1.CHECK “L” TERMINAL CIRCUIT (SHORT)

1. Turn ignition switch OFF.
2. Disconnect alternator connector.
3. Turn ignition switch ON.

Does charge warning lamp illuminate?
YES>>GO TO 2.
NO>>Refer to Work Flow.
2.CHECK HARNESS CONTINUITY (SHORT CIRCUIT)

1. Turn the ignition switch OFF.
2. Disconnect the battery cable from the negative terminal.
3. Disconnect combination meter connector.
4. Check continuity between combination meter harness connector and ground.

Combination meter harness connector | Ground | Continuity
Connector No. | Terminal No.
M53 | 28 | Not existed

Is the inspection result normal?
YES>>Replace combination meter.
NO>>Repair the harness.