1.CHECK AMBIENT SENSOR

1. Turn the ignition switch OFF.
2. Remove the ambient sensor. Refer to Exploded View.
3. Check the resistance between the ambient sensor terminals. Refer to the applicable table for the normal value.

   Terminal | Condition | Resistance: kΩ
   Temperature: °C (°F)
   1 | 2 | −15 (5) | 12.73
   −10 (14) | 9.92
   −5 (23) | 7.80
   0 (32) | 6.19
   5 (41) | 4.95
   10 (50) | 3.99
   15 (59) | 3.24
   20 (68) | 2.65
   25 (77) | 2.19
   30 (86) | 1.81
   35 (95) | 1.51
   40 (104) | 1.27
   45 (113) | 1.07

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the ambient sensor.