DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1716 | [PRESSDATA ERR] FL | Malfunction in the tire pressure data from the front left wheel transmitter. |

- Transmitter ID registration incomplete
- Transmitter malfunction

C1717 | [PRESSDATA ERR] FR | Malfunction in the tire pressure data from the front right wheel transmitter.
C1718 | [PRESSDATA ERR] RR | Malfunction in the tire pressure data from the rear right wheel transmitter.
C1719 | [PRESSDATA ERR] RL | Malfunction in the tire pressure data from the rear left wheel transmitter.

DTC REPRODUCTION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Drive for 10 minutes at a speed of 40 km/h (25 MPH) or more.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1716”, “C1717”, “C1718”, or “C1719” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END