- The axis B feed pressure solenoid valve is installed on the actuator control module and builds up the source pressure for the gear operation actuators for odd number gears and reverse gear and for the clutch B pressure solenoid valve based on the signals from TCM. The solenoid valves adjust the source pressure to drive the gears and clutches.
- The axis B feed pressure solenoid valve is a N/L type (normal low) in which no control oil pressure is built up when no current flows through the coil.