JUDGMENT STANDARD

Damage grade | Judgment standard | Example of specific operation | Remarks
A |

- There is damage to frame parts.
- Replacement of door opening parts
- Damage to the extent that the roof replacement is necessary

- Replacement of member
- Replacement of sill
- Replacement of lock pillar
- Replacement of front pillar
- Replacement of roof
- Replacement of floor
- Replacement of inner wheelhouse
- Replacement of rear fender
- Replacement of front-end module (radiator core support)
- Replacement of windshield glass, side window glass, rear window glass, door glass

NISSAN recommend ″Certified body shop″ for structural body repair.

- Damage of aluminum die-casting parts
  (Other than door)

- Removal, installation, and replacement of rear seatback support
- Replacement of strut housing

B |

- Sheet metal and replacement of bolt-on outer plate parts
- Partial sheet metal and paint of outer plate

- Replacement, sheet metal, and paint of front fender
- Replacement, sheet metal, and paint of hood
- Replacement, sheet metal, and paint of door
- Replacement, sheet metal, and paint of trunk lid
- Replacement, sheet metal, and paint of rear panel
- Sheet metal and paint of rear fender
  (Outer plate damage only)
- Sheet metal and paint of roof
- Replacement, repair, and paint of bumper
- Replacement, repair, and paint of center mud guard
- Replacement, repair, and paint of pillar garnish
- Replacement, repair, and paint of door mirror
- Replacement of undercovers

—

JUDGMENT PROCEDURE
The judgment procedures for framework are exampled as per the following.

Location | Judgment procedure
Body shop | Check with device |

- Check the dimensions described in the body repair manual using tracking gauge.
- Check damage of aluminum die-casting parts by the dye penetrant testing procedure.

Body shop and workshop | Driving and visual check point |

- If the vehicle can be driven, check that the steering position.
  → There is possible structural damage if it drifts to the left or right.
- If the vehicle can be driven, check the straightness by the driving check.
  → There is possible structural damage if it drifts to the left or right.
- Check for signs of interference between tire and fender protector around the damaged area.
  → There is possible structural damage if there are signs of interference.
- Check for impact and damage around front pillar.
  → It is possible that the damage influences the door fitting accuracy.