COMBINATION METER

- The buzzer (1) for the warning chime system is integrated in the combination meter.
- The combination meter sounds the alarm buzzer installed in the combination meter when receiving the signal from various units and switches.

BCM
BCM receives signals from various units and switches, and transmits the buzzer output signal to the combination meter via CAN communication if it judges that the warning buzzer should be activated.
BCM warning function list

Warning functions | Signal name
Light reminder warning chime |

- Position light request signal
- Door switch signal (driver side)

Seat belt warning chime | Seat belt buckle switch signal (driver side)
Reverse warning chime (For Canada) | Shift position signal