1.CHECK SELF-DIAGNOSIS Perform self-diagnosis for “ABS” with CONSULT-III. Is the inspection result normal? YES>>GO TO 2. NO>>Check items displayed by self-diagnosis.
2.CHECK COMBINATION METER
Check that the lamp illuminates for approximately 2 seconds after the ignition switch is turned ON.
Is the inspection result normal?
YES>>Replace ABS actuator and electric unit (control unit). Refer to Exploded View (GT-R certified NISSAN dealer).
NO>>Repair or replace combination meter.