Removal

1.Remove drive belt. Refer to Exploded View.

- Keep auto‐tensioner pulley arm locked after drive belt is removed.

2.Remove auto‐tensioner and idler pulley.

- Keep auto‐tensioner pulley arm locked to install or remove auto‐tensioner.

Installation
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Check drive belt is securely installed around all pulleys.
- Check drive belt is correctly engaged with the pulley groove.
- Check for engine oil and engine coolant are not adhered drive belt and pulley groove.