1.CHECK INFORMATION DISPLAY

1. Start engine.
2. Press MAIN switch on ASCD steering switch.
3. Drive the vehicle at more than 40 km/h (25 MPH)
   ■ CAUTION ■
   Always drive vehicle at a safe speed.
4. Press SET/COAST switch.
5. Check that the readings of the speedometer show the same values as the set speed indicated in the information display while driving the vehicle on a flat road.

Is the inspection result normal?
YES>>INSPECTION END
NO>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).