1.TRANSMITTER ID REGISTRATION PROCEDURE With CONSULT-III.

1. Turn the ignition switch ON.
2. Display the “WORK SUPPORT” screen and select “ID REGIST”.
3. Select the start button on the “ID REGIST” screen.
4. Press the transmitter activation tool (J-45295) (1) against the side of the tire at the location closest to the transmitter.
5. Wait until the indicator lamp turns off (approximately 5 seconds).
   ■ CAUTION ■
   Perform the ID registration procedure starting from the vehicle front left wheel, then repeat the procedure in the order of the front right wheel, rear right wheel, and rear left wheel.
6. When ID registration is completed, check the following pattern at each wheel.

   Sequence | ID registration position | Turn signal lamp | CONSULT-III
   1 | Front left wheel | 2 blinks | “Red” ↓ “Green”
   2 | Front right wheel
   3 | Rear right wheel
   4 | Rear left wheel

7. After the ID registration procedure for all wheels is completed, press “END” to end ID registration, and check that ID registration for all wheels is completed.

Is the check result normal?
YES>>ID registration END.
NO>>Performs trouble-diagnosis of the Tire Pressure Monitoring System (TPMS). Refer to Diagnosis Description (GT-R certified NISSAN dealer).