1.CHECK OUTPUT SHAFT SPEED SENSOR CIRCUIT Refer to Diagnosis Procedure (GT-R certified NISSAN dealer). Is the inspection result normal? YES >>GO TO 2. NO >>Repair or replace damaged parts.
2.CHECK LINE PRESSURE SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 3.
NO >>Repair or replace damaged parts.
3.CHECK CLUTCH A PRESSURE SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 4.
NO >>Repair or replace damaged parts.
4.CHECK CLUTCH B PRESSURE SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 5.
NO >>Repair or replace damaged parts.
5.CHECK SLEEVE A1 POSITION SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 6.
NO >>Repair or replace damaged parts.
6.CHECK SLEEVE A2 POSITION SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 7.
NO >>Repair or replace damaged parts.
7.CHECK SLEEVE B11 POSITION SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 8.
NO >>Repair or replace damaged parts.
8.CHECK SLEEVE B12 POSITION SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 9.
NO >>Repair or replace damaged parts.
9.CHECK SLEEVE B2 POSITION SENSOR CIRCUIT
Refer to Diagnosis Procedure (GT-R certified NISSAN dealer) and Diagnosis Procedure (GT-R certified NISSAN dealer).
Is the inspection result normal?
YES >>GO TO 10.
NO >>Repair or replace damaged parts.
10.CHECK HARNESS BETWEEN TCM AND GROUND

1. Turn ignition switch OFF.
2. Disconnect TCM harness connectors.
3. Check continuity between TCM vehicle side harness connector terminal and ground.

   TCM vehicle side harness connector | Ground | Continuity
   Connector | Terminal
   B45 | 3 | Ground | Existed
   4
   7
   8

Is the inspection result normal?
YES>>GO TO 11.
NO >>Repair or replace damaged parts.
11.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
Is the inspection result normal?
YES >>Replace TCM. Refer to Exploded View (GT-R certified NISSAN dealer).
NO >>Repair or replace damaged parts.