DTC DETECTION LOGIC

DTC | Display Item | Malfunction detected condition | Possible causes
C1730 | FLAT TIRE FL | Front left wheel pressure is 70 kPa (0.7 kg/cm2, 10 psi) or less | Low tire pressure
C1731 | FLAT TIRE FR | Front right wheel pressure is 70 kPa (0.7 kg/cm2, 10 psi) or less
C1732 | FLAT TIRE RR | Rear right wheel pressure is 70 kPa (0.7 kg/cm2, 10 psi) or less
C1733 | FLAT TIRE RL | Rear left wheel pressure is 70 kPa (0.7 kg/cm2, 10 psi) or less
NOTE：
Specified tire pressure = 200 kPa (2.0 kg/cm2, 29 psi)

DTC REPRODUCTION PROCEDURE
1.CHECK DTC DETECTION
With CONSULT-III

1. Drive for 3 minutes at a speed of 40 km/h (25 MPH) or more, then drive normally for 10 minutes.
2. Perform self-diagnosis of the low tire pressure warning control unit.

Is DTC “C1730”, “C1731”, “C1732”, or “C1733” detected?
YES>>Perform trouble diagnosis. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END