COMPONENT DESCRIPTION

Component | Function
Suction filter | Removes foreign matter contained in fluid and prevents them from entering the hydraulic circuit
Inline filter
Heat exchanger |

- Cools down fluid with the water-cooled cooler
- When the engine starts at low temperature, warms fluid quickly with heated coolant

Front control module | Oil pump | Sucks fluid accumulated in the oil pan to build up oil pressure in the circuit
Valve | Line pressure valve |

- Controls the line pressure
- The line pressure is adjusted by the line pressure solenoid

Clutch A solenoid valve | Controls the clutch pressure of clutch A/B
Clutch B solenoid valve
Lubricating flow valve |

- Controls the lubricating flow
- The lubricating flow is adjusted by the lubricating flow solenoid

Clutch lubricating switching valve | Switches the lubricating distribution of the clutch.
Pressure sensor | Clutch A pressure sensor | Detects the clutch pressure of clutch A/B
Clutch B pressure sensor
Actuator control module | Valve | Axis A feed pressure valve |

- Controls the feed pressure of axis A/B
- Each feed pressure is adjusted by the axis A/B feed pressure solenoid

Axis B feed pressure valve
Shift solenoid valve 1 | Controls 4 shift actuator pistons by combining ON and OFF of each shift solenoid valve and switching the sequence valve circuit
Shift solenoid valve 2
Shift solenoid valve 3
Shift solenoid valve 4
Sequence valve
Pressure sensor | Line pressure sensor | Detects the line pressure