REMOVAL

1.Remove the bolts (A) and (B) tighten the rear diffuser together with the rear of rear wheel house protector.

2.Remove the bolt (A) tighten the rear diffuser (2) together with the front of rear wheel house protector (1).

3.Remove the clip (A) connecting the center mud guard with the rear wheel house protector.

4.Remove the clips of rear wheel house protector, and then remove it from the wheel house.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Replace the mounting bolts with new ones to prevent electric corrosion when removing the rear diffuser mounting bolt.
- Tighten the bolts of the rear wheel house protector and the rear diffuser to the specified torque. Refer to Exploded View.