1.CHECK METER CONTROL SWITCH INPUT SIGNAL

1. Turn the ignition switch ON.
2. Measure voltage between the following terminals of the combination meter.

   Terminal No. | Condition | Voltage (Approx.)
   23 – 6 | When switch is pressed | 0 V
   Other than the above | 5 V
   24 – 6 | When switch is pressed | 0 V
   Other than the above | 5 V
   25 – 6 | When trip A/B reset switch is pressed | 0 V
   Other than the above | 5 V
   26 – 6 | When enter switch is pressed | 0 V
   Other than the above | 5 V
   27 – 6 | When select switch is pressed | 0 V
   Other than the above | 5 V

Is the inspection result normal?
YES>>INSPECTION END
NO>>GO TO 2.
2.CHECK METER CONTROL SWITCH SIGNAL CIRCUIT

1. Turn the ignition switch OFF.
2. Disconnect the connectors of combination meter and meter control switch.
3. Check for continuity between the combination meter harness connector terminal and the meter control switch harness connector.

   Combination meter | Meter control switch | Continuity
   Connector | Terminal | Connector | Terminal
   M53 | 6 | M54 | 2 | Existed
   23 | 3
   24 | 1
   25 | 8
   26 | 6
   27 | 7

4. Check for continuity between the combination meter harness connector and the ground.

   Combination meter | Ground | Continuity
   Connector | Terminal
   M53 | 6 | Not existed
   23
   24
   25
   26
   27

Is the inspection result normal?
YES>>INSPECTION END
NO>>Repair the harnesses or connectors.