REMOVAL

1.Remove the front seat. Refer toRemoval and Installation.

2.Remove the seat cushion outer finisher (2). Referto Disassembly and Assembly.

3.Remove the power seat switch knob.

4.Remove the screws (A).

5.Remove the power seat switch (1) from the seat cushion outer finisher.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- When performing the work, use shop cloths to protect the parts from damage.
- Always fix the harness clamp in the normal position.