NOTE： Check the headlamp (HI) circuit if the headlamp (HI) is not turned ON. Refer to Component Function Check. ■ CAUTION ■ Before performing the diagnosis, check that the headlamp (HI) bulb is normal. 1.CHECK DAYTIME RUNNING LIGHT OPERATION CONSULT-III ACTIVE TEST

1. Select “DAYTIME RUNNING LIGHT” of BCM (HEADLAMP) active test item.
2. With operating the test items, check that daytime running light operation.

   On | : Daytime running light ON
   Off | : Daytime running light OFF

Is the daytime running light turned ON/OFF?
YES>>Daytime running light relay circuit is normal.
NO>>Refer to Diagnosis Procedure.