DISASSEMBLY NOTE： For any parts other than filler plug, remove and replace only when a trace of oil leakage is detected. Be careful of the following items when removing the component parts.

- Drain the transmission oil before removing the 3rd-5th check pin. Refer to Draining.
- Stop the engine with the shift lever in the P position before removing the 3rd-5th check pin.

ASSEMBLY
Be careful of the following items when installing the component parts.
■ CAUTION ■

- Never reuse filler plug gasket.
- Never reuse plain washer.
- Never reuse O-ring.
- Apply the transmission oil when installing the O-ring.
- Temporarily tighten by hand, and then tighten to the specified torque when installing the parts to the transmission assembly.

- Fill with the transmission oil after installation. Refer to Filling.