DTC DETECTION LOGIC

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0705 | Transmission range sensor "A" circuit malfunction (PRNDL input) | A DTC is set if either of the following statuses is detected consecutively.

1. Any of the range sensors No. 0, No. 1, No. 3, or No. 5 is stuck to OFF.
2. Any of the range sensors other than those detected in 1 above is stuck to OFF.

- Range sensor
- Harness or connector
  (Open or shorted in the range sensor circuit)

A DTC is set if either of the following statuses is detected consecutively.

1. Either of the range sensors No. 2 or No. 4 is stuck to OFF.
2. Any of the range sensors other than those detected in 1 above is/are stuck to OFF.

A DTC is set if 2 or more of the following sensors and switch are stuck to ON or OFF consecutively: Range sensors No. 0, No. 1, No. 2, No. 3, No. 4 or No. 5, and park position switch. |

- Range sensor
- Park position switch
- Harness or connector
  (Open or shorted in the range sensor circuit)
  (Open or shorted in the park position switch circuit)

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Start the engine.
2. Shift the shift lever as per the following: P→R→N→A positions (Keep the shift lever for 5 seconds or more at each position).
3. Shift the shift lever as per the following: A→N→R→P positions (Keep the shift lever for 5 seconds or more at each position).
4. Repeat the procedure shown in 2 and 3 above 2 times.
5. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Start the engine.
2. Shift the shift lever as per the following: P→R→N→A positions (Keep the shift lever for 5 seconds or more at each position).
3. Shift the shift lever as per the following: A→N→R→P positions (Keep the shift lever for 5 seconds or more at each position).
4. Repeat the procedure shown in 2 and 3 above 2 times.
5. Check self-diagnosis.

Is DTC P0705 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident.