CHECK CLEARANCE BETWEEN BODY AND STEERING MEMBER

1. | Upper rear hoodledge (RH) | 2. | Shim | 3. | Steering member
A. | Passenger side | B. | Clearance | C. | Measuring point

1.Tighten the driver side steering member mounting bolts to the specified torque. Refer to Exploded View (GT-R certified NISSAN dealer).
■ CAUTION ■
Install the steering member with the shim assembled if the shim is installed between the upper rear hoodledge (RH) and steering member when removing the steering member.

2.Measure the clearance between upper rear hoodledge (RH) and steering member using a feeler gauge.

- Perform the measurement at the 4 measuring points.

  Standard | : 0 – 0.6 mm

- Select the shim from the table below so that the clearance is within the standard if it is outside the standard. Then, install it between upper rear hoodledge (RH) and steering member.

  Measuring result (mm) | Shim thickness (mm) | Shim part number
  0.7 – 1.2 | 0.6 | 31438 JF00A
  1.3 – 1.6 | 1.2 | 31438 JF00B
  1.7 – 2.3 | 1.6 | 31438 JF00C
  2.4 – 3.4 | 2.3 | 31438 JF00D

3.Install the passenger side steering member mounting bolts after checking that the values are within the standard.