DTC DETECTION LOGIC ■ CAUTION ■

- Before TCM is replaced, the IP characteristics must be extracted, based on the information read out from the malfunctioning TCM. For reading out the IP characteristic data, refer to “CONSULT-III GT-R TCM CONFIGURATION MANUAL”.
- If no IP characteristic data can be extracted TCM and the transmission assembly must be replaced as a set.

DTC | Self-diagnosis name | DTC detection condition | Possible cause
P0607 | Control module performance | DTC is set if TCM performance malfunction is detected due to malfunction of analogue/digital conversion and self shut-down system, or reset failure at CPU malfunction detection. | TCM

DTC CONFIRMATION PROCEDURE
1.PREPARATION BEFORE OPERATION
If another “DTC CONFIRMATION PROCEDURE” is performed just before the next test, turn the ignition switch OFF and wait for 10 seconds or more, then perform the next test.
>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE
With CONSULT-III

1. Turn ignition switch OFF, and wait for 5 seconds or more.
2. Turn the ignition switch ON and wait for 5 seconds or more, then turn it OFF again.
3. Repeat the procedure shown in 1 and 2 above 32 times.
4. Turn the ignition switch ON.
5. Check “Self Diagnostic Result” of “TRANSMISSION”.

Without CONSULT-III

1. Turn ignition switch OFF, and wait for 5 seconds or more.
2. Turn the ignition switch ON and wait for 5 seconds or more, then turn it OFF again.
3. Repeat the procedure shown in 1 and 2 above 32 times.
4. Turn the ignition switch ON.
5. Check self-diagnosis.

Is DTC P0607 detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>Go to Intermittent Incident