ADJUSTMENT OF STEERING ANGLE SENSOR NEUTRAL POSITION ■ CAUTION ■ To adjust neutral position of steering angle sensor, make sure to use CONSULT-III. (Adjustment cannot be done without CONSULT-III) 1.ALIGN THE VEHICLE STATUS Stop the vehicle with front wheels in the straight-ahead position.
>>GO TO 2.
2.PERFORM THE NEUTRAL POSITION ADJUSTMENT FOR THE STEERING ANGLE SENSOR

1. Select “ABS”, "WORK SUPPORT" and “ST ANGLE SENSOR ADJUSTMENT" in order with CONSULT-III.
2. Select “START”.
   ■ CAUTION ■
   Never touch steering wheel while adjusting steering angle sensor.
3. After approximately 10 seconds, select “END”.
4. Turn ignition switch OFF, then turn it ON again.
   ■ CAUTION ■
   Always perform the above operation.

>> GO TO 3.
3.CHECK DATA MONITOR

1. Run the vehicle with front wheels in the straight-ahead position, then stop.
2. Select “ABS”, “DATA MONITOR” and “STR ANGLE SIG” in order with CONSULT-III, and check steering angle sensor signal.

   STR ANGLE SIG | : 0±2.5°

Is the steering angle within the specified range?
YES>>GO TO 4.
NO>>Perform the neutral position adjustment for the steering angle sensor again, GO TO 1.
4.ERASE THE SELF-DIAGNOSIS MEMORY
Erase self-diagnosis memories for “ABS” with CONSULT-III. Refer to CONSULT-III Function (GT-R certified NISSAN dealer).
Are the memories erased?
YES>>INSPECTION END
NO>>Check the items indicated by the self-diagnosis.