1.CHECK HAZARD SWITCH SIGNAL BY CONSULT-III CONSULT-III DATA MONITOR

1. Turn the ignition switch ON.
2. Select "HAZARD SW" of BCM (FLASHER) data monitor item.
3. With operating the hazard switch, check the monitor status.

Monitor item | Condition | Monitor status
HAZARD SW | Hazard switch | While pressing the switch | On
While not pressing the switch | Off

Is the item status normal?
YES>>Hazard switch circuit is normal.
NO>>Refer to Diagnosis Procedure.