TCM uses 3 different power supply routes to distribute power supply to each sensor.

Sensor power supply 1 | Sensor power supply 2 | Sensor power supply 3

- Output shaft speed sensor
- Line pressure sensor

- Clutch A pressure sensor
- Clutch A speed sensor
- 6th-Neutral position sensor
- 2nd-4th position sensor
- Range sensor power supply 1 (Range sensor No. 0, 1, 3, 5)

- Clutch B pressure sensor
- Clutch B speed sensor
- 1st-Reverse position sensor 1
- 1st-Reverse position sensor 2
- 3rd-5th position sensor
- Range sensor power supply 2 (Range sensor No. 2, 4)