REMOVAL Pull up and remove engagement with body from trunk lid weather-strip joint. ■ CAUTION ■ Never pull strongly the trunk lid weather-strip during removal. INSTALLATION

1.Working from the upper section, align the center of trunk lid weather-strip with vehicle center mark and install weather-strip.

2.Engage the trunk lid weather-strip with the vehicle body.
■ CAUTION ■

- Securely fit each corner.
- Pull trunk lid weather-strip lightly to check for looseness.