DTC DETECTION LOGIC

DTC | Display item | Malfunction detected condition | Possible cause
P1826 | OIL TEMP SEN | Malfunction of transmission oil temperature sensor signal has been detected. | Malfunction of transmission fluid temperature sensor or transmission fluid temperature sensor circuit.

DTC CONFIRMATION PROCEDURE
1.DTC REPRODUCTION PROCEDURE
With CONSULT-III

1. Turn the ignition switch ON.
2. Erase self-diagnostic results for “ALL MODE AWD/4WD”.
3. Start the engine and run idle for 8 minutes or more.
4. Perform self-diagnosis for “ALL MODE AWD/4WD”.

Is DTC “P1826” detected?
YES>>Proceed to diagnosis procedure. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END.
■ CAUTION ■
If “CAN COMM CIRCUIT [U1000]” is detected, first perform the trouble diagnosis for CAN communication line. Refer to Diagnosis Procedure (GT-R certified NISSAN dealer).