1.CHECK SUNLOAD SENSOR

1. Turn the ignition switch ON.
2. Check the input voltage from the sunload sensor between the A/C auto amp. harness connector and ground. Refer to the applicable table for the normal value.

   (+) | (−)
   A/C auto amp. | —
   Connector | Terminal
   M66 | 15 | Ground

   NOTE：
   - When checking indoors, use a lamp of approximately 60 W. Move the lamp towards and away from the sensor to check.
   - The sunload amount produced by direct sunshine in fair weather is equivalent to approximately 0.77 kW/m2 (660 kcal/m2·h).

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace the sunload sensor.