1.CHECK STOP LAMP SWITCH

1. Turn the ignition switch OFF.
2. Disconnect stop lamp switch harness connector.
3. Check the continuity between stop lamp switch harness connector terminals.

   Stop lamp switch | Condition | Continuity
   Terminal
   1 – 2 | Release stop lamp switch (When brake pedal is depressed) | Existed
   Push stop lamp switch (When brake pedal is released) | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace stop lamp switch. Refer to Exploded View.