1.CHECK TRUNK LID OPENER SWITCH

1. Turn ignition switch OFF.
2. Disconnect trunk lid opener switch connector.
3. Check continuity between trunk lid opener switch terminals.

   Terminal | Condition | Continuity
   Trunk lid opener switch
   1 | 2 | Trunk lid opener switch | Pressed | Existed
   Released | Not existed

Is the inspection result normal?
YES>>INSPECTION END
NO>>Replace trunk lid opener switch. Refer to Removal and Installation.