1.INSPECTION START

1. Turn ignition switch ON.
2. Check “Self diagnostic result” with CONSULT-III.
3. Touch “ERASE”.
4. Perform DTC Confirmation Procedure.See DTC Logic.

Is the DTC B260F displayed again?
YES>>GO TO 2.
NO>>GO TO 3.
2.REPLACE ECM
Replace ECM. Refer to Special Repair Requirement (GT-R certified NISSAN dealer).
>>INSPECTION END
3.CHECK INTERMITTENT INCIDENT
Refer to Intermittent Incident.
>>INSPECTION END