DTC DETECTION LOGIC NOTE：

- If DTC P0460 is displayed with DTC UXXXX, first perform the trouble diagnosis for DTC UXXXX.
- If DTC P0460 is displayed with DTC P0607, first perform the trouble diagnosis for DTC P0607. Refer to DTC Logic (GT-R certified NISSAN dealer).

When the vehicle is parked, naturally the fuel level in the fuel tank is naturally stable. It means that output signal of the fuel level sensor does not change. If ECM senses sloshing signal from the sensor, fuel level sensor malfunction is detected.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
P0460 | Fuel level sensor circuit noise | Even though the vehicle is parked, a signal being varied is sent from the fuel level sensor to ECM. |

- Harness or connectors
  (The CAN communication line is open or shorted)
- Harness or connectors
  (The sensor circuit is open or shorted)
- Combination meter
- Fuel level sensor

DTC CONFIRMATION PROCEDURE
1.PRECONDITIONING
If DTC Confirmation Procedure has been previously conducted, always perform the following procedure before conducting the next test.

1. Turn ignition switch OFF and wait at least 10 seconds.
2. Turn ignition switch ON.
3. Turn ignition switch OFF and wait at least 10 seconds.

>>GO TO 2.
2.PERFORM DTC CONFIRMATION PROCEDURE

1. Start engine and wait maximum of 2 consecutive minutes.
2. Check 1st trip DTC.

Is 1st trip DTC detected?
YES>>Go to Diagnosis Procedure (GT-R certified NISSAN dealer).
NO>>INSPECTION END