DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B1042 B1043 B1044 B1045 B1046
B1047
CONTROL UNIT
Air bag diagnosis sensor unit is malfunctioning or out of the specification

- Malfunction in air bag diagnosis sensor unit
- Configuration in air bag diagnosis sensor unit does not match the vehicles specification

DTC CONFIRMATION PROCEDURE
1.CHECK SELF-DIAG RESULT
With CONSULT-III

1. Turn ignition switch ON.
2. Perform “AIR BAG” Self Diagnostic Result.

Without CONSULT-III

1. Turn ignition switch ON.
2. Check the air bag warning lamp status. Refer to Air Bag Warning Lamp Diagnosis.

NOTE：
SRS does not enter diagnosis mode if no malfunction is detected in user mode.
Is malfunctioning part detected?
YES>>Refer to Diagnosis Procedure.
NO>>INSPECTION END