×: ON –: OFF
Condition | VDC OFF indicator lamp
Ignition switch OFF | –
For 2 second after turning ignition switch ON (Under the normal system condition) | ×
2 second later after turning ignition switch ON | –
OFF mode is selected by set-up switch (VDC) (VDC function is OFF) | ×
VDC/TCS is malfunctioning. | ×
ABS is malfunctioning. | ×
EBD is malfunctioning. | ×
Hill start assist is malfunctioning. | ×