1.CHECK SELF-DIAGNOSTIC RESULT-1

1. Perform “Self-diagnostic result” of BCM using CONSULT-III.
2. Erase DTC.
3. Perform DTC Confirmation Procedure. Refer to DTC Logic.

Is DTC 2195 detected?
YES>>GO TO 2.
NO>>INSPECTION END
2.CHECK EQUIPMENT OF THE VEHICLE
Check that unspecified accessory part related to engine start is not installed.
Is unspecified accessory part related to engine start installed?
YES>>GO TO 3.
NO >>Replace BCM. Refer to Removal and Installation.
3.CHECK SELF-DIAGNOSTIC RESULT-2

1. Obtain the customers approval to remove unspecified accessory part related to engine start, and then remove it.
2. Perform “Self-diagnostic result” of BCM using CONSULT-III.
3. Erase DTC.
4. Perform DTC Confirmation Procedure. Refer to DTC Logic.

Is DTC 2195 detected?
YES>>Replace BCM. Refer to Removal and Installation.
NO>>INSPECTION END