CONSULT‐III APPLICATION ITEMS

Test item | Diagnosis mode | Description
BUZZER | Data Monitor | Displays BCM input data in real time.
Active Test | Operation of electrical loads can be checked by sending driving signal to them.

DATA MONITOR

Display item [Unit] | Description
PUSH SW [On/Off] | Status of push button ignition switch judged by BCM.
UNLK SEN‐DR [On/Off] | Status of unlock sensor judged by BCM.
VEH SPEED 1 [Km/h] | Value of vehicle speed signal received from ABS actuator and electric unit (control unit) with CAN communication line.
KEY SW‐SLOT [On/Off] | Status of key slot judged by BCM.
TAIL LAMP SW [On/Off] | Status of each switch judged by BCM using the combination switch readout function.
FR FOG SW [Off] | This item is displayed, but cannot be monitored.
DOOR SW‐DR [On/Off] | Status of driver side door switch judged by BCM.

ACTIVE TEST

Display item [Unit] | Description
IGN KEY WARN ALM | The key warning chime operation can be checked by operating the relevant function (On/Off).
SEAT BELT WARN TEST | The seat belt warning chime operation can be checked by operating the relevant function (On/Off).
ID REGIST WARNING | The ID regist warning chime operation can be checked by operating the relevant function (On/Off).
LIGHT WARN ALM | The light warning chime operation can be checked by operating the relevant function (On/Off).
REVERSE WARNING | The reverse warning chime operation can be checked by operating relevant function (On/Off).