- The range sensors are installed on the A/T shift selector and the park position switch on the transmission, detecting the shift lever position.
- TCM recognizes the shift lever position by combining signals from 6 range sensors used for the range position recognition and park position switch.

TCM recognized position | Shift lever position | Park position switch | Range sensor
No. 0 | No. 1 | No. 2 | No. 3 | No. 4 | No. 5
P | P | ON | ON | OFF | OFF | OFF | OFF | OFF
R | R | OFF | OFF | ON | ON | OFF | OFF | OFF
N | N | OFF | OFF | OFF | ON | ON | ON | OFF
A/M | A/M | OFF | OFF | OFF | OFF | OFF | ON | ON