OIL LEVEL DISPLAY After mounting/removing of battery or combination meter, the combination meter power supply is cut off temporarily. Therefore, the engine oil amount data may be erased from the combination meter, causing the oil level to be not displayed. Refer to System Description for the condition that the combination meter reads the resistance of oil level sensor.
AMBIENT AIR TEMPERATURE
For the ambient air temperature display, the value is displayed on the information display after the signal from ambient sensor is corrected by the combination meter. Therefore, the indication value may not match the actual ambient air temperature. Refer to System Description for details on the correction process.
POSSIBLE DRIVING DISTANCE
The calculated distance to empty may differ from the actual distance to empty if the refueling amount is approximately 15 (4 US gal, 3-1/4 lmp gal) or less. This is because the refuel control (moves the fuel gauge needle quicker than normal judging that the driver is refueling the vehicle) is not performed in such a case.