REMOVAL

1.Remove the clip connecting the floor under cover and the fender protector (LH/RH) (rear). Refer to Exploded View.

2.Remove the bolt (front under cover rear edge) tightened together with the front under cover.

3.Remove the floor under cover mounting bolts.

4.Remove the floor under cover.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- To prevent electric corrosion, always check bolts and washers for surface treatment peeling and white rust corrosion when mounting bolts of Spec V floor undercover are removed.
- If surface treatment is peeled off, bolts and washers are reusable when contact surfaces between washer and carbon parts are painted using touch-up paint.Never reuse bolts or washers when white rust corrosion is detected.
- Always tighten the mounting bolts to the specified torque.