1.CHECK INTELLIGENT KEY Check Intelligent Key. Refer to Component Function Check. Is the inspection result normal? YES>>GO TO 2.
NO>>Repair or replace the malfunctioning parts.
2.CHECK COMBINATION METER DISPLAY FUNCTION
Check combination meter display function.
Refer to Component Function Check.
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CONFIRM THE OPERATION
Confirm the operation again.
Is the result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.