1.CHECK SELF DIAGNOSIS RESULT Perform “COMBINATION METER” self diagnostic result. Refer to CONSULT-III Function (METER/M&A) Is DTC detected? YES>>Repair or replace the malfunctioning parts. NO>>GO TO 2.
2.CHECK POWER SUPPLY
Check fuse are not blown.
Check ignition power supply of combination meter. Refer to Diagnosis Procedure
Is the inspection result normal?
YES>>GO TO 3.
NO>>Repair or replace the malfunctioning parts.
3.CHECK SEAT BELT BUCKLE SWITCH CIRCUIT (DRIVER SIDE)
Check seat belt buckle switch circuit (driver side). Refer to Component Function Check
Is the inspection result normal?
YES>>GO TO 4.
NO>>Repair or replace the malfunctioning parts.
4..CHECK SEAT BELT BUCKLE SWITCH CIRCUIT (PASSENGER SIDE)
Check seat belt buckle switch circuit (passenger side). Rer to Component Function Check
Is the inspection result normal?
YES>>GO TO 5.
NO>>Repair or replace the malfunctioning parts.
5..CHECK SEAT BELT WARNING LAMP CIRCUIT
Check seat belt warning lamp circuit. Rer to Diagnosis Procedure
Is the inspection result normal?
YES>>GO TO 6.
NO>>Repair or replace the malfunctioning parts.
6.CONFIRM THE OPERATION
Confirm the operation again.
Is the inspection result normal?
YES>>Check intermittent incident. Refer to Intermittent Incident.
NO>>GO TO 1.