1.PERFORM ECM RE-COMMUNICATING FUNCTION

1. Install ECM.
2. Insert the registered Intelligent Key (*2), turn ignition switch to “ON”.*2: To perform this step, use the key that has been used before performing ECM replacement.
3. Maintain ignition switch in the “ON” position for at least 5 seconds.
4. Turn ignition switch to “OFF”.
5. Start engine.

Can engine be started?
YES>>Procedure is completed.
NO>>Initialize control unit. Refer to CONSULT-III Operation Manual NATS-IVIS/NVIS.