DTC DETECTION LOGIC

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B260B | STEERING LOCK UNIT | BCM detects malfunctioning of steering lock unit before steering unlocking. | Steering lock unit

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Press the push-button ignition switch, when steering is locked.
2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END