REMOVAL

1.Remove battery cover.

2.Disconnect the battery cable from the negative terminal.

3.Remove cover of battery positive terminal.

4.Remove harness mounting nuts (1) and fusible link holder mounting nut (2).

5.Disconnect harness connectors (3) and remove battery terminal with fusible link (4).

INSTALLATION
Install in the reverse order of removal.

Harness mounting nut
: 13.2 N·m (1.3 kg-m, 10 ft-lb)
Fusible link holder mounting nut
: 13.2 N·m (1.3 kg-m, 10 ft-lb)