REMOVAL

1.Remove the front diffuser. Refer to Exploded View.

2.Drain the transmission oil from the transmission assembly. Refer to Draining.

3.Remove the oil pan mounting bolt (), and then remove the oil pan (1) and oil pan gasket.

| : Front of vehicle

4.Remove the magnet (1) from the oil pan.

INSTALLATION
Note the following, and install in the reverse order of removal.
■ CAUTION ■

- Clean foreign matter (gear wear particles) that are adhered on the inside of the oil pan and on the magnet, and then assemble.
- Completely wipe out any moisture, oil and old gasket from the gasket mounting surface.
- Never reuse oil pan gaskets.
- Never forget assembly of drain tube.
- Never reuse drain plug. In addition, install new drain plug after adjustment of transmission oil filling.

- When the oil pan is installed, tighten bolts in the order shown in the figure after temporarily tightening the oil pan mounting bolt.

  | : Front of vehicle

- Fill with the transmission oil to the transmission assembly after installation. Refer to Filling.