DTC DETECTION LOGIC NOTE：

- If DTC B2601 is displayed with DTC U1000, first perform the trouble diagnosis for DTC U1000. Refer to DTC Logic.
- If DTC B2601 is displayed with DTC U1010, first perform the trouble diagnosis for DTC U1010. Refer to DTC Logic.

DTC No. | Trouble diagnosis name | DTC detecting condition | Possible cause
B2601 | SHIFT POSITION | BCM detects when a difference between the shift P input signal and the shift position signal received from IPDM E/R via CAN communication continues for 2 seconds or more |

- Harness or connectors
  (A/T shift selector circuit is open or shorted)
- A/T shift selector (detention switch)

DTC CONFIRMATION PROCEDURE
1.PERFORM DTC CONFIRMATION PROCEDURE

1. Turn ignition switch ON under the following conditions, and wait for at least 2 seconds.

- Shift lever is in the P position.
- Do not depress the brake pedal.

2. Check “Self diagnostic result” with CONSULT-III.

Is DTC detected?
YES>>Go to Diagnosis Procedure.
NO>>INSPECTION END