REMOVAL ■ CAUTION ■ Never drop or strike yaw rate/side/decel G sensor or use power tool etc., because yaw rate/side G sensor is sensitive to the impact.

1.Remove rear console. Refer to Exploded View.

2.Disconnect yaw rate/side/decel G sensor harness connector.

3.Remove mounting bolts. Remove yaw rate/side/decel G sensor.

INSTALLATION
Note the following items, and install in the reverse order of removal.
■ CAUTION ■

- Never drop or strike yaw rate/side/decel G sensor or use power tool etc., because yaw rate/side/decel G sensor is sensitive to the impact.
- After work, always calibrate of decel G sensor. Refer to Description (GT-R certified NISSAN dealer).